LLT OF CSMA /CD

# PROCEDURE:

\* It is technique where different situations that follow this protocol

\*check if the sender is ready for transmitting data packets

\*sender has to keep on checking if the transmission link is idle

\*transmit the data and check for collisions

\* if no collision was detected in propogation ,the sender completes its frame

Transmission and resets the counters

